MATERIAL SAFETY DATA SHEET

1. PRODUCT IDENTIFICATION

Product Name : PETRO FLEXIA 15W-40

Manufacturer : PT. PETROMITRA PACIFIC INTERNUSA

Address : JL. Raya Serpong No.26B

Telephone Number : 021- 5312 5632

Application : Engine Oil

1. COMPOSITIONAL INFORMATION

Chemical Name CAS # OSHA PEL ACGIH TLV %(Range)

Petroleum Oil 64742-54-7 \_ \_ 90 – 100

1. HAZARDS IDENTIFICATION

Hazard Classification: Harmful if swallowed. Inhalation causes headaches, dizziness,

drowsiness and nausea, cause eye and skin irritation

1. FIRST AID MEASURES

Inhalation : Remove to fresh air. If effects persist, seek treatment by a doctor.

Skin Contact : Wash skin with water immediately. Get medical attention if any

symptoms develop. To remove the material from skin, apply a

waterless hand cleaner, mineral oil, or petroleum jelly. Then wash with

soap and water.

Ingestion : Do not induce vomiting. Wash mouth out with water. Obtain

immediate treatment by a doctor and provide a copy of this sheet.

Eyes : Flush eyes immediately with fresh water for 15 minutes while holding

the eyelids open. Get immediate medical attention.

1. FIRE FIGHTING MEASURES

Flash Point, 0C : 230

Extinguishing Media : Dry chemical, Foam or CO2

Special Fire Fighting Procedures : For firefighter involving this material, do not enter any

enclosed orconfined fire space without proper protective

equipment, including self contained breathing apparatus.

Combustion Products : Oxides of carbon.

1. ACCIDENTAL RELEASE MEASURES

Personal Precautions : Immediately contact emergency personnel. Use suitable

Protective equipment. Follow all fire fighting procedures.

Environment Precautions : Prevent liquid entering sewers, drains or water courses.

Decontamination : Absorb in earth or sand or other suitable material. In case

of spillage on water contain by a boom and collect by

skimming or absorption.

1. HANDLING & STORAGE

Handling : Do not ingest. Avoid contact with skin, eyes and clothing.

Wash thoroughly after handling

Storage : Keep containers tightly closed. Keep container in a cool,

well ventilated area. Do not cut, grind, drill, weld, reuse or

dispose of containers unless adequate precautions are

taken against these hazards.

1. EXPOSURE CONTROLS / PERSONAL PROTECTION

Occupational Exposure Limits : None assigned.

Engineering Control Measures : Provide exhaust ventilation. Ensure that eyewash stations

and safety showers are close to the work station location.

Chemical splash goggles. Wear suitable protective clothing

and gloves

Personal Protection : for eyes.

1. PHYSICAL & CHEMICAL CHARACTERISTICS

Appearance and odor : Brown liquid and characteristic odor

Density @ 15oC : 0.8890

Boiling Point (oC) : Not determined

Melting point (oC) : Not applicable

Pour Point : -24

Flash Point, oC : 208

Solubility in water Non

Vapour Density (air=1) : Not determined

Evaporation rate : Not determined

(Butyl Acetate=1)

1. STABILITY AND REACTIVITY

Stability : Stable under normal condition

Conditions to Avoid : Avoid exposure to extreme heat

Material to Avoid : Strong Oxidizing Agent

Hazardous Decomposition : Oxides of Carbon

1. TOXICOLOGICAL INFORMATION HEALTH EFFECT

On eyes : May cause temporary irritation and discomfort

On skin : Generally non irritant on incidental contact. Excessive or

Prolonged contact may give rise to slight irritation.

By inhalation : High concentration of mist may give rise to respiratory irritation.

By ingestion : Ingestion of large quantities may cause nausea, sickness and

diarrhoea.

Chronic Toxicity : No hazard anticipated

Other : Products which have become contaminated might present more

serious health effect.

1. ECOLOGICAL INFORMATION

Ecotoxicity : NA.

Biodegradability : Not readily biodegradable but inherently biodegradable.

Leaching and penetration through surface soils is generally

regarded as resulting in long term persistence.

Other Ecological Information : Spillages may penetrate the soil causing ground water

contamination. Fresh or used product may harmful to

aquatic life.

1. DISPOSAL CONSIDERATIONS

Waste information : Avoid contact of spilled material and runoff with soil and

Surface waterways. Consult an environmental professional

to determine if local, regional or national regulations

would classify spilled or contaminated materials as

hazardous waste. Use only approved

transporters, recyclers, treatment, storage or disposal

facilities.

Dispose method : Dispose of in accordance with all applicable Local and

national regulations.

1. OTHER INFORMATION

Other Information : The data and advice given apply when the product is sold

for the stated application (s). The product is not sold as

suitable for any other application. Use of the product for

applications other than as stated in

this sheet may give rise to risk not mentioned in this sheet.

Should not use the product other than for the stated

application or applications without seeking advice from

us. If you have purchased the product for supply to a third

party for use at. work, it is your duty to take all necessary

steps to secure that any person handling or using the

product is provided with the information in this sheet.

If you are an employer, it is your duty to tell your

employees and others

who may be affected of any hazard described in this sheet

and of any precautions which should be taken